**Warmflow Unvented Cylinder Ecodesign End-of-Life Information**

**Commission Regulation (EU) No 813/2013**

**End-of-Life Information**  
Warmflow Unvented Cylinders must be disposed of according to local regulations by using a public or private waste collection service.

**Safety Risks**  
Prior to disassembly, the appliance should be electrically isolated and disconnected.

Any fluids within the appliance must be drained, and disposed of in-line with local regulations.

Care should be taken when handling the appliance due to weight, use appropriate PPE and lifting aids.

Polyisocyanurate foam insulation – suitable PPE should be used for respiration protection, and to avoid skin or eye contact.  
  
**Disassembly of the Product**  
The main materials of the components are:

* Mild Steel
* Stainless Steel
* Polyisocyanurate Foam
* Plastic Components
* Electronic Components

These may be recycled – depending on the local recycling facilities available.  
  
The appliance is assembled by using mechanical fasteners and can be disassembled with standard tools.

The components of a typical appliance are shown below (not all components may be fitted, depending on appliance specification)

**Casing and key components**



101

111

9

8

7

5

6

1

4

3

2

|  |  |  |  |
| --- | --- | --- | --- |
| Item | Description | Main Materials | Special Notes |
| 1 | Casing | Coated Galvanised Steel |  |
| 2 | T&P Relief Valve | Plastic, Brass | Consult Component Manufacturer |
| 3 | Foam Insulation | Polyisocyanurate Foam | Wear Appropriate PPE |
| 4 | Storage Tank | Stainless Steel |  |
| 5 | Thermostat Housing | Plastic, Copper, Electronic Components |  |
| 6 | Immersion Heater | Brass, Incoloy, Electronic Components | Consult Component Manufacturer |
| 7 | Casing Top | Plastic |  |
| 8 | Heating Coils | Stainless Steel |  |
| 9 | Dip Pipe | Stainless Steel |  |
| 10 | Solar Coil | Stainless Steel |  |
| 11 | Casing Base | Plastic |  |
| Others | Expansion Vessel | Steel, Rubber, Brass | Consult Component Manufacturer |

Various other brackets, fasteners and components may be used, with up to 5% of appliance weight